Product Specification Guide
Vari-Green Control – Remote Dial

Remote Dial shall be a Vari-Green control specifically designed to provide 0-10 volt DC signal to 
Greenheck’s Vari-Green Motor.