Product Specification Guide
Vari-Green Control – Two Speed
 
Two Speed control shall be a Vari-Green Control specifically designed to allow the Vari-Green Motor to operate at two discreet speeds.  Two Speed control shall include two dials that may be set at any point between 0 and 10 volts DC and an integral transformer capable of reducing 115/208-240 volt AC power to 24 volt AC power.